24VAC





**Outlet**

**Relay**

**Pin 5**

**Inlet**

**Relay**

**Pin 6**

**Manual**

**Flush Button**

**Outlet**

**Solenoid**

**Inlet**

**Solenoid**






10K

**Outlet Sol. Open**

**LED**

**Inlet Sol. Open**

**LED**





**‘Reading’**

**LED**

Network

9VDC

P

P

LOW

HIGH



22K

BC548C

22K

BC548C

b

e

c

b

e

c



470Ω

220Ω

470Ω

220Ω

-

S

+

-

S

+